**New Product—Automotive Ground Strap**

Crane Cams Ignition has released a new Automotive Ground Strap to help eliminate the most likely problem for ignition systems—insufficient chassis ground. It’s a simple fact, you can’t have enough grounds in the car to ensure trouble-free operation. This high quality, tin-plated, copper braid ribbon cable is a full 24”, reaching from cylinder head, battery, or ignition to frame. All Digital CD ignitions are known for their sensitivity to RF noise. This new cable can help by providing proper ground connections.

***Features:***

***• 24” Total Length***

***• Tin Plated Copper Flexible Braid Gives Maximum Grounding Capability***

***• #10 AWG Braid***

***• 3/8 Stud Tin Plated Copper Eyelets***

***• Heat Sleeve Covering Crimp for Tight, Clean Finish***

***• Part Number 6000-6720***

***Download High Resolution Image Files at www.AutoPressReleases.com***